Sarah Wood

Embedded Programming

BeagleBone Black

C11-B1

Run the GTK+, "Hello World" example on pp. 436-437.

To do this correctly, you must open a VNC connection as shown on the bottom of p. 434. Compile the code as shown on p. 437 and run the program, ./gtksimple.

Once this has been done, using the same procedure, complete the GTK+ temperature sensor example on pp. 438-439.

Submit a screen captures of the code running and a copies of the code.