Sarah Wood

Embedded Programming

BeagleBone Black

C6-B2

Grove Cape

In the /exploringBB/chp06/GPIO directory on your BBB, modify the simple.cpp code to run using a Grove cape.

Use the J6(GPIO2) socket for the LED, and J2(GPIO14) for the button. This [documentPreview the documentView in a new window](https://owatc.instructure.com/courses/273503/files/48383219/download?wrap=1) will help. Use [vimView in a new window](https://owatc.instructure.com/courses/273503/files/48383188/download?wrap=1) or any editor you're familiar with to open and modify the code.  When you have made these changes, re-build the code and execute. You should see the LED flash. Submit your code.